|  |  |  |  |
| --- | --- | --- | --- |
| **Contact:** | Putzmeister Holding GmbH  Marketing  Max-Eyth-Str. 10  72631 Aichtal, Germany  Tel.: +49 (0)7127 599 311  Fax: +49 (0)7127 599 140  E-mail: [marketing@putzmeister.com](mailto:marketing@putzmeister.com) | **Press release no.:**  **Date:**  **Author:** | 2036  10.02.2025  Marketing |

**Putzmeister showcases the manoeuvrable and versatile entry-level model M27-4 PL at Bauma**

M27-4 PL truck-mounted concrete pump – largest reach on two axles

**Aichtal, February 2025 – At Bauma 2025, Putzmeister presents a machine which will delight European customers: With a reach of almost 27 metres on two axles, it combines a wide range of applications with comfortable manoeuvrability. The new small-sized model from Putzmeister is on show from Monday 7 April to Sunday 13 April at the Putzmeister stand in Hall B6 at Bauma.**

The M27-4 Performance Line truck-mounted concrete pump from Putzmeister impresses with short delivery times thanks to the standard design and an unbelievable price-performance ratio, among other things. The entry-level model on two axles is very compact with its small wheelbase and thus easy to manoeuvre. However, it is also available on three axles for markets where a low axle load is required. With its comprehensive basic configuration, the Putzmeister truck-mounted concrete pump is approved for Europe. It is therefore extremely attractive as an entry-level model particularly for European customers who do not want to do without an impressive reach of 27 metres.

The M27-4 is in its element here: on smaller construction sites, when pouring concrete from base plates, in urban areas, when concreting bridges, in special or hose applications.

**Compact, lightweight design for additional manoeuvrability and payload**

The M27-4 is characterised by a compact and lightweight design. This offers not only good manoeuvrability of the truck-mounted concrete pump, but also allows the longest placing boom to be transported on two axles.

The robust TRC substructure is equipped with hydraulic telescopic legs, which allow simple and stable installation of the machine.

A 3.1 metre long continuous platform and the modular storage concept ensure a high storage volume. The assembly of attachments is very simple and there is sufficient space available for containers, shelves or storage compartments. Accessibility to all relevant components also makes the work easier.

**Infinitely variable support** **for diverse jobs**

The fully flexible, infinitely variable support is the optimal solution for almost every construction site as it offers the ideal combination of support area and boom reach. Ergonic ® 3 and iSC light (intelligent Set-up Control) make possible a variety of positions – from zero to full support. The safety system reduces the extent of supports significantly, without compromising stability.

**Flexible reach for a wide range of applications**

The 4-arm boom with compact Z fold system is even more flexible and easy to use due to the 100° A angle and the overextension. With a 26.4 metre reach and 22.5 metre horizontal reach, as well as an unfolding height of 6.7 metres, the machine can be used for a variety of applications.

**Ergonomics and safety for working optimally**

Standard with the 27-4: a high degree of safety thanks to the T0 support, which is located under the continuous platform, large steps and a clever lighting concept. There is also the container that can be lowered hydraulically to the correct working height, a handrail, the safety shutdown at the hopper and lots more.

**Ergonic® 3 – control for increased user friendliness**

Ergonic® 3 offers simple, quick and safe handling of the machine, as is the case with all Putzmeister products. In particular, the intuitive operation with a clear menu structure and logical arrangement of the functions on the display ensures efficient working and quick reactions. The complete overview of the machine status (incl. valves, sensors, LEDs on fuses) guarantees comprehensive control. And also the detailed error management allows the machine operator to quickly identify and eliminate faults – often without the need for a Putzmeister technician.

Multilevel emergency operation guarantees the functionality of the machine even in tough conditions and in almost every situation.

**Performance Line means top-class equipment as standard**

The M27-4 PL comes with a Putzmeister concrete pump 11 H and thus with an output of 110 m3/h and 78 bar concrete pressure. The equipment leaves almost nothing to be desired and also includes the Ergonic® control with cable remote control; 2-layer delivery lines, a vibrator, 500 l water tank, control point lighting, the folding spray guard, a central pressure gauge, folding side panels on both sides, a high-pressure cleaner, underride protection at the rear, Connected Services and lots more.

**About the Putzmeister Group**

﻿The Putzmeister Group develops and produces machinery of high technological quality in the fields of concrete conveying, truck-mounted concrete pumps, stationary concrete pumps, placing booms and accessories, plant technology, conveying industrial high-density solids through pipes, concrete spraying and transport in tunnels and below ground, mortar machines, plastering machines, screed conveying, injection and specialist applications. Market segments are the construction industry, mining and tunnel construction, major industrial projects, power and sewage treatment plants as well as waste incineration plants worldwide.

The company is based in Aichtal, Germany. With over 4000 employees, the company achieved a turnover of 1 billion euros in the 2023 financial year.