|  |  |  |  |
| --- | --- | --- | --- |
| **Contact:** | Putzmeister Mörtelmaschinen GmbH  Marketing  Max-Eyth-Str. 10  72631 Aichtal, Germany  Tel.: +49 (0)7127 599 0  Fax: +49 (0)7127 599 140  E-mail: [mm@putzmeister.com](mailto:mm@putzmeister.com) | **Press release no.:**  **Date:**  **Author:** | 2055  10.03.2025  Märkert/Schlösinger |

The Putzmeister EstrichBoy DC 260 makes a successful comeback at bauma

The legend lives on: The completely redesigned EstrichBoy classic – the DC 260

Aichtal, February 2025 – The new EstrichBoy DC 260 is yet another logical development of the legendary classic from the Putzmeister brand, Brinkmann. The main focus of its redevelopment was on user-friendliness, durability and ease of servicing. With numerous, practical configuration options, it is equipped for all requirements on the construction site and cuts an impressive figure thanks to its outstanding efficiency and cost-effectiveness. From Monday 7th April to Sunday 13th April, visitors can experience the EstrichBoy’s comeback live at bauma in Munich in Hall B6.

More functional, easier to maintain and service, less complicated: The new EstrichBoy is impressive across the board. It pumps all earth-moist floor screeds – for instance cement screed, calcium sulphate screed (anhydrite), magnesia screed or vibration-laid tiling (depending on consistency). Its high output ensures that it is enormously efficient. The high-quality “made in Germany” technology is complemented by first-class service with a comprehensive dealer service network and practical machine operator and technician training courses at the Putzmeister Academy.

**As strong as the DC260/45 – even stronger than the DC260/55**

The new EstrichBoy is available in two motor versions: The DC260/45 model, with its economical three-cylinder Deutz TD 2.2 L3, offers 36.4 kW of power and a maximum delivery rate of 5 m3/h. The DC260/55 model is the more powerful alternative, achieving 44.5 kW of power and a maximum delivery rate of 5.2 m3/h. In addition, both motorised machines are available in version B, which is equipped with a loader, and version BS, which boasts both a loader and a scraper. With the BluePower option, the motor speed can be set to one of five levels. The display shows whether fuel is being saved or whether the maximum power of the EstrichBoy is being employed.

All machine versions meet the applicable Stage V emissions standard and strict noise protection requirements, making them well prepared for the future. As a result, the EstrichBoy can therefore be used anywhere in the EU and Switzerland. And as it complies with TRGS 554, it can also be operated in (partially) enclosed areas such as underground car parks without any problems.

With a towing load of just 1900 kg in the version with a loader and scraper, the EstrichBoy DC 260 is the lightest screed conveyor in its power class on the market. This gives machine operators more options when selecting tractor units. A lifting eye for easily relocating the machine on the construction site using a crane is also installed as standard.

**Clear, robust, and easier to operate than ever before**

The operating concept has been completely overhauled and makes operation even simpler. All operating and display elements have been arranged centrally in one place, ensuring the machine operator has everything in view at all times. The combination of robust switches and the proven keypad combines the advantages of both operating systems and is therefore ideally suited to the requirements of day-to-day work on the construction site. This enables easy and intuitive operation of the machine and effectively prevents operating errors and, as a result, avoids machine downtimes.

The high-resolution display, including a USB port for software updates, is a completely new design. Protected by armoured glass and resistant to dirt, it has been designed to withstand the rigorous demands of everyday life on the construction site. During the development process, the focus was on creating a clear display and straightforward, logical menu navigation. New service menus provide additional information and increase ease of operation.

**Even more options, even more possibilities**

An optional feature is the telematics system which increases efficiency and uptime thanks to online monitoring of key operating and machine parameters, in particular through remote access by Putzmeister service staff in the event of a fault.

The integrated anti-theft protection system provides additional security. Other options include a working light with powerful LEDs, a silo structure, a truck coupling or a polystyrene hopper for the D and DB(S) models for easy metering of loose polystyrene bulk material.

**Safe in every respect: Mixing apparatus with reverse rotation**

The hydraulic mixing apparatus can be operated in reverse as required. This is a practical solution if the mixing apparatus or a mix is stuck. A pressure limiting valve ensures reliable overload protection at all times.

**Saves time and effort: Carefully considered maintenance concept**

Maintenance and services are crucial for every screed conveyor. For this reason, particular attention was paid to ensuring that all important service and maintenance points are easily accessible on the EstrichBoy EC 260. The well-thought-out body concept, with an enlarged hood opening angle along with a removable rear section and removable floor panels, makes it easier to access the motor compartment, thereby saving time during service work. Since the operating panel is permanently installed, servicing and commissioning can be easily carried out with the hood open.

Meanwhile, instead of being mechanically driven, the mixing apparatus is now fully hydraulic – meaning that belt changes and adjustments are a thing of the past. Cleaning the radiator has now become significantly easier, too, as both the inside and outside are easily accessible for cleaning in just a few steps.

**About EstrichBoy and the Brinkmann brand**

The Brinkmann brand has been part of the Putzmeister Group since 2002. The machines have been continuously maintained and further developed by Putzmeister since the takeover. The EstrichBoy product brand has been established on the market for almost 60 years and represents exceptionally high-quality screed conveyors.

**About Putzmeister Mortar Machines**

Putzmeister Mortar Machines GmbH is part of the Putzmeister Group and specialises in the development and production of mortar machines and screed pumps. The applications covered range from cement screed, self-levelling floor screed and plaster to shotcrete, fine concrete and other special applications. Putzmeister Mortar Machines includes the brands Putzmeister, Brinkmann and Lancy. Products are manufactured at the company headquarters in Aichtal, Germany, and in Floirac (near Bordeaux) in France.

**About the Putzmeister Group**

﻿The Putzmeister Group develops and produces machinery of high technological quality in the fields of concrete conveying, truck-mounted concrete pumps, stationary concrete pumps, placing booms and accessories, plant technology, conveying industrial high-density solids through pipes, concrete spraying and transport in tunnels and below ground, mortar machines, plastering machines, screed conveying, injection and specialist applications. Market segments are the construction industry, mining and tunnel construction, major industrial projects, power and sewage treatment plants as well as waste incineration plants worldwide.

The company is based in Aichtal, Germany. With over 4000 employees, the company achieved a turnover of 1 billion euros in the 2023 financial year.